The shield designed for this project was a shield for using on a standard formatted Arduino board, whether Arduino UNO, MEGA or YUN, to be able of making tests of the HomeChef oven from GOR prior to the realization of the first SandS motherboard. 

Also, this design was created as a plan B, in case there were too many issues in pursuing a design making use of the Dogstamp module for communications, in which case it should be possible to use any other Arduino board running a Software Serial algorithm to communicate in the non-branded scenario.

Note: there is no v02 of the design, it was made in parallel with the SandS motherboard, which means there were two different design rounds of this device, once when the motherboard was manufactured for the first time and another one for the third iteration of the design.
