Compilation:
	gcc *.c -o executable
Prerequisites:
	connected host board (mainboard/shield host) must be running the "configurator" sketch
Running:
	executable [device]
	Windows:   executable COM*:
	Linux:     executable /dev/ttyACM*:
	Mac:       executable /dev/tty.usbmodem*
